Install 2 – 1.25 Innerduct along the East side of Monticello LN N roughly 774’ South at 35-38’ from CL.

South to Intersection of Monticello Ln and 85th Ave N (Cty Rd 109), Then along the N Side of 85th Ave N (Cty Rd 109) for 858’ to the West Side of Jefferson HWY at roughly 57-60 N of Centerline. Proceed along the West side of Jefferson at 42-45ft Tapering down to 37-40 after the turn lane ends on the West of Centerline HWY 600’ to the Osseo City Limits.

